//***************** C-Media AC97 NT4 driver Release Note ******************//
                       (Support ALI(sis7018+Ali5451 )

2002/10/01
-   Unify the codec's output string to "C-Media AC97 xxxx" (ex. Mixer/Wave Out/Stereo In/Midi Out).
-   Fixed a bug: Mic Boost enable function.
-   Fixed a bug: Cmi9739: Master/Waveout volume control.
-Fixed a bug: Moving Waveout Volume when Mater volume is mute on Cmi9739.

2002/08/19
Version: 4.10.00.0008b
-   Adjust Volume's gain value

Date: 2002/08/02
Version: 4.10.00.0007b
-   Fixed a bug: Master Volume Constrol

2002/07/30
Version: 4.10.00.0006b
-   Fixed a bug: Move the balance of master volume to left and CD-In's to right most, it should be silence.

2002/07/12
Version: 4.10.00.0005b
-   Let silence if the scale of Internal CD-In/ Line-In is setting to min.

2002/06/03
Version: 4.10.00.0004b
   Default Master volume is set to Max(0xffff), 
           WaveOut, CD-Outn, Line-Out is the half of max(0x7fff),
	   Mic-In, CD-In, Line-In is 0x1fff.

2002/05/28
Version: 4.10.00.0003b
--  Enable Master volume boost function.

2002/05/21
Version: 4.10.00.0002b

Driver description:
  The C-Media cm9738 driver is working on the NT4.0 with Ali5451 and Sis7018 chipsets. 
  It consists three files:
  IAC97U4.DLL	// ac97 user mode driver 
  IAC97K4.SYS	// ac97 kernel mode driver
  OEMSETUP.INF	// installation inforamtion
----------------------------
