; Copyright (c) 1997-1999, Sony Corporation
;;
;; SonyPI.inf
;;  Sony Programmable I/O Control
;;
;;  (C) 1999,2000 Sony Corporation All rights reserved.
;;
;;  06/28/2000
;;
;;  Revision 1.03

;--------- Version Section ---------------------------------------------------

[Version]
Signature = "$CHICAGO$"
Class = System
ClassGUID = {4d36e97d-e325-11ce-bfc1-08002be10318}
Provider = %ProviderName%
CatalogFile = sonypi.cat
DriverVer=08/01/2000,6.0.5.06280Q

[ControlFlags]
ExcludeFromSelect=*SNY6001

;--------- SourceDiskNames and SourceDiskFiles Section -----------------------

; These sections identify source disks and files for installation.  They are
; shown here as an example, but commented out.

[SourceDisksNames.x86]
1 = %DiskId%,,,

[SourceDisksFiles]
SonyPI.sys  = 1
SonyPI.dll = 1
;;SonyPI.inf = 1

;--------- DestinationDirs Section -------------------------------------------

[DestinationDirs]
DefaultDestDir=10
SPI_Files_Driver = 10,System32\Drivers
SPI_Files_DLL = 10,System
;;SPI_Files_INF = 10,Inf


;--------- Manufacturer and Models Sections ----------------------------------

[Manufacturer]
%MfgName%=Mfg0

[Mfg0]
%DeviceDesc%=SPI_DDI, *SNY6001

;---------- DDInstall Sections -----------------------------------------------
; --------- Windows 9X -----------------

[SPI_DDI]
;;CopyFiles=SPI_Files_Driver, SPI_Files_DLL, SPI_Files_INF
CopyFiles=SPI_Files_Driver, SPI_Files_DLL
AddReg=SPI_9X_AddReg

[SPI_9X_AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SonyPI.sys
HKR, "Parameters", "BreakOnEntry", 0x00010001, 0

; --------- Windows NT -----------------

[SPI_DDI.NT]
;;CopyFiles=SPI_Files_Driver, SPI_Files_DLL, SPI_Files_INF
CopyFiles=SPI_Files_Driver, SPI_Files_DLL
AddReg=SPI_NT_AddReg

[SPI_DDI.NT.Services]
Addservice = SPI, 0x00000002, SPI_AddService

[SPI_AddService]
DisplayName    = %SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\SonyPI.sys

[SPI_NT_AddReg]
HKLM, "System\CurrentControlSet\Services\SPI\Parameters",\
	"BreakOnEntry", 0x00010001, 0

; --------- Files (common) -------------

[SPI_Files_Driver]
SonyPI.sys

[SPI_Files_DLL]
SonyPI.dll

;;[SPI_Files_INF]
;;SonyPI.inf


;--------- Strings Section ---------------------------------------------------

[Strings]
ProviderName="Sony Corporation"
MfgName="Sony Corporation"
;DeviceDesc:DeviceManager
DeviceDesc="Sony Programmable I/O Control Device"
;DeviceClassName="SPIC"
SvcDesc="Sony Programmable I/O Conrtol Device"
DiskId="SonyPI"



